¼o’kZ 2017&18½

uxj fuxe nsgjknwu ds cYyqiqj pkSd ls x<h dSUV dSuky jksM esa vUMj xzkmUM dsfcy] fo|qr iSuy vkfn fo|qr dk;Z djkus

gsrq

fufonk izi=

fufonk izi= ewY;& :0 1000-00

th0,l0Vh0&18 izfr”kr vfrfjDr

fufonk izi= cspus dh frfFk%&fnukad 28-07-2017 ls 11-08-2017 vijkgu 1%00 cts rd

fufonk vkaeU=.k dh frfFk%& fnukad 14-08-2017 lka; 3%00 cts rd Vw&fcM ds vk/kkj ij rduhdh o foRrh; fcM vkaefU=r dh tkrh gSA

fufonk [kksyus dh frfFk fnukad 16-08-2017 izkr% 10%30 cts rduhdh fcM esa lQy fufonknkrkvksa dh gh foRrh; fcM [kksyh tk;sxhA

uxj fuxe] nsgjknwu

uxj fuxe] nsgjknwuA

fufonk izi=

:0 1000+18 izfr”kr

th0,l0Vh0 izfr fufonk

VSfDudy fcM

cYyqiqj pkSd ls x<h dSUV dSuky jksM esa vUMj xzkmUM dsfcy@taD”ku ckWDl o iSuy cksMZ yxkus vkfn fo|qr dk;Z lEcU/khA

1. ljdkj }kjk ekU;rk izkIr “,” Js.kh ds fo|qr Bsdsnkj dk izek.k i= nsuk gksxkA
2. bUde VSDl] th0,l0Vh0] iSu uaEcj nsuk gksxk rFkk xr nks o’kksZa dk vk;dj fjVuZ Hkh nsuk gksxkA
3. lEiw.kZ dk;Z dh nks o’kZ rd fu%”kqYd eSUVsusUl djuh gksxh rFkk vUMj xzkmUM dsfcy fdlh Hkh dkj.ko”k {kfrxzLr gksus ij Bsdsnkj }kjk gh Bhd@cnyuh gksxhA
4. dsfcy gSoYl] ikSyhdSc] ikbZeu , Js.kh dk yxkuk gksxkA
5. ,e0lh0ch0@,e0lh0lh0ch0@dkUVsDVj@VkbZej@gSoYl],y0,.MVh0]yhxjsUV vkfn dh yxkuh gksxhA
6. foxr nks o’kksZa dk VuZ vksoj :0 50 yk[k ds fo|qr lEcfU/kr dk;ksZa dk izek.k i= nsuk gksxkA
7. rduhdh fcM o foRrh; fcM vyx&vyx fyQkQs esa nsuh gksxh] ftl ij rduhdh o foRrh; fcM fy[kk gksxk rFkk nksuks fcMksa dks ,d cMs fyQkQs esa lhy cUn djds nsuk gksxkA
8. rduhdh fcM esa lQy gksus okys fufonknkrk dh gh foRrh; fcM [kksyh tk;sxhA
9. fufonk izfrHkwfr /kujkf”k rhu izfr”kr dh lh0Mh0vkj0@,Q0Mh0vkj0 nks o’kksZa dh oS|rk ds lkFk ofj’B foRr vf/kdkjh] uxj fuxe nsgjknwu ds uke VSfDudy fcM ds lkFk nsuh vfuok;Z gS] vU;Fkk fufonk ij fopkj ugh fd;k tk;sxkA
10. fufonk Lohd`r gksus ij fufonk jkf”k :0 05 izfr”kr dk;ZiwfrZ izfrHkwfr ds :i esa tek djuk gksxkA
11. fdlh Hkh o leLr fufonk dks fcuk djk.k crk;s fujLr djus dk vf/kdkj uxj vk;qDr nsgjknwu esa fufgr gksxkA
12. dk;Z iw.kZ gksus ij fujh{kd fo|qr lqj{kk ls izek.k i= ysuk gksxk ftldk dksbZ “kqYd uxj fuxe nsgjknwu }kjk ugh fn;k tk;sxkA
13. fufonk vkbZVe okbZl nj vk/kkfjr nh tk;sxhA
14. fdlh Hkh foHkkx esa dkyh lwph esa ntZ u gksus dk “kiFk i= nsuk gksxkA

vf/k”kklh vfHk;Urk

uxj fuxe] nsgjknwuA

**Schdule-B (Financial Bid)**

**Supply / Laying & Dismentling Street light under ground cable at Ballupur Chowk to Garhi cantt (Canal road) Dehradun**.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| S.No | Item | P.S No | Qty | Rate | Amount |
| 1 | Supply and laying of aluminium conductor P.V.C insulated armoured,served, sheathed cable 1100 Volts grade at a depth of 750 mm blow ground lavel a cushion of 75mm thick sand around and protected with burnt bricks on side and on top on surface the cable shall be fixed on M.S clamp etc. Of suitable size or as directed by the engineer-incharge, complete in all respect. The armouring of the cable shall be properly connected with the earth conductor by clamp etc (m) (i) 25 sq.mm. 3.5 core cat. A. | 5101 | 3000 mtr |  |  |
| 2 | Supply and laying of aluminium conductor P.V.C insulated armoured, served, sheathed cable 1100 Volts grade on surface the cable shall be fixed on M.S clamp etc. Of suitable size or as directed by the engineer- incharge, complete in all respect. Include of suitable size support G.I pipe. (m) (i) 50 sq.mm. 3.5 core cat. A. | 5102(b)(i) | 100 mtr |  |  |
| 3 | Providing Plinth for pole with 1:3:6 Cement conerect complete in all respect.. | As per P.W.D Ar rate | 83 no |  |  |
| 4 | Supply & fixing of Street light feeder pole box made of C.R.C.A Sheet complete with M.C.B & locking arangement. | As per P.W.D Ar rate | 83 no |  |  |
| 5 | Supply and fixing of Street light timer box with 100 amp MCCB, 2 no 100 amp contactor and 24 hour timer switch. | MR | 4 no |  |  |
| 6 | Painting of pole with coat of aluminium paint over red oxide complete in all respect. | As per P.W.D Ar rate | 83 no |  |  |
| 7 | Supply & burying of G.I rod of 4.5 m long and 40 mm dia. By driving it vertically inside the ground for its full length with top at least 0.6m below the ground level with G.I. wire of 5mm dia, support 16mm dia. 32 mm long G.I. bolt with washer G.I. lug welded to G.I. for earthing etc. complete in all respects. MR | As per P.W.D rate 5.1 | 4 no |  |  |
| 8 | Supply & fixing of aluminum lug 25 sqmm | 5108 | 664 no |  |  |
| 9 | Supply & fixing of brass nikil gland 25 sqmm. | 5106(E) | 166 no |  |  |
| 10 | Supply & Laying D.W.C Pipe 50 mm dia | As per MR rate | 2500 mtr |  |  |
|  |  |  |  | Total |  |

vf/k”kklh vfHk;Urk]

uxj fuxe] nsgjknwuA