e;wj fogkj fLFkr odZ”kkWi esa dsfcy] iSuy o ok;fjxa lEcfU/k fo|qr dk;Z

¼o’kZ 2015&16½

gsrq

fufonk izi=

fufonk izi= ewY; :0 500-00++13-50 VSDl

fufonk izi= foØ; dh frfFk%&fnukad 18-05-15 ls 01-06-15 nksigj 1%00 cts rd

fufonk vkaeU=.k dh frfFk%& fnukad 02-06-15 lka; 3%00 cts rd

fufonk [kksyus dh frfFk %& fnukad 02-06-15 lka; 4%00 cts

uxj fuxe] nsgjknwu

uxj fuxe] nsgjknwuA

fufonk izi=

:0 500-00+13-5 izfr”kr

lfoZl VSDl izfr fufonk

VSfDudy fcM

e;wj fogkj fLFkr odZ”kkWi esa dsfcy] iSuy o ok;fjxa lEcfU/k fo|qr dk;Z

1. ljdkj }kjk ekU;rk izkIr “,” Js.kh ds fo|qr Bsdsnkj dk izek.k i= nsuk gksxkA
2. bUde VSDl] lsy VSDl] iSu uaEcj nsuk gksxk rFkk xr nks o’kksZa dk vk;dj fjVuZ Hkh nsuk gksxkA
3. lEiw.kZ dk;Z dh ,d o’kZ rd fu%”kqYd eSUVsusUl djuh gksxhA
4. dsfcy gSoYl] ikSyhdSc] ikbZeu dk yxkuk gksxkA
5. ,e0lh0ch0@,e0lh0lh0ch0@dkUVsDVj vkfn gSoYl] ,y0 ,.M Vh0 dh yxkuh gksxhA
6. foxr nks o’kksZa dk VuZ vksoj :0 nl yk[k ds fo|qr lEcfU/kr dk;ksZa dk izek.k i= nsuk gksxkA
7. rduhdh fcM o foRrh; fcM vyx&vyx fyQkQs esa nsuh gksxh rFkk nksuks fcMksa dks ,d cMs fyQkQs esa lhy cUn djds nsuk gksxkA
8. rduhdh fcM esa lQy gksus okys fufonknkrk dh gh foRrh; fcM [kksyh tk;sxhA
9. fufonk izfrHkwfr /kujkf”k :0 8500-00 dh lh0Mh0vkj0@,Q0Mh0vkj0 ,d o’kZ dh oS|rk ds lkFk ys[kkf/kdkjh uxj fuxe nsgjknwu ds uke VSfDudy fcM ds lkFk nsuh vfuok;Z gS] vU;Fkk fufonk ij fopkj ugh fd;k tk;sxkA
10. fufonk Lohd`r gksus ij fufonk jkf”k :0 5 izfr”kr dk;Z iwfrZ izfrHkwfr ds :i esa tek djuk gksxkA

vf/k”kklh vfHk;Urk

uxj fuxe] nsgjknwuA

Nagar Nigam Dehradun.

Schedule-

Name OF Work:- Cable laying, Pannel Box & other wiring work at Mayur Vihar Work Shop.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Sr No. | Description | Unit | Qty | Rate | Amount |
| 1 | Errection of Pole 9mtr long with CC, painting of pole etc. | Each | 4 |  |  |
| 2 | Supply and Errection of Stayset, complete in all respect. | Each | 2 |  |  |
| 3 | Supply and fixing of suitable size MS Clamp for fixing of insulators, complete in all respect. | Set | 6 |  |  |
| 4 | Supply and fixing of PVC seathed, armoured cable of size 3 sqmm 3.5 core on wall, pole as required. | Mtr | 200 |  |  |
| 5 | Supply and Fixing of 7/16 Stay wire for support of LT armoured cable of size 3.5x35 sqmm. | Mtr | 200 |  |  |
| 6 | Point wiring of Light point/ Fan point in PVC conduit on surface.(Sch) 80283 | Each | 20 |  |  |
| 7 | Wiring for circuit/ submain wiring along with earth wire with 2x4 sqmm+ 1x2.5 sqmm Cu wire. | Mtr | 100 |  |  |
| 8 | Wiring for light/ power plug with 2x4 sq. mm FR PVC insulated copper conductor.  Single core cable in surface/ recessed PVC conduit along with 1 N0 4 sq. mm FR  PVC insulated copper conductor single core cable for loop earthing as required. | Mtr | 50 |  |  |
| 9 | Supply and Fixing of DP MCB 32 Amp with MS Enclosure. | Each | 5 |  |  |
| 10 | Supply and Fixing of SP MCB DB Double Door 8 way. (80519) (Sch) | Each | 2 |  |  |
| 11 | Supply and Fixing of SP MCB 6-32 Amp in existing DB.(Sch) 80567 | Each | 12 |  |  |
| 12 | Supply and Fixing of 200 amp ICTPN switch, with angle iron frame for fixing. | Each | 1 |  |  |
| 13 | Earthing with G.I earth plate 600 mm x 600 mm x 6 mm thick including accessories, and providing masonry enclosure with cover plate etc, complete in all respect. (80593)(80595)(Sch) with charkol and salt | Each | 3 |  |  |
| 14 | Supply and laying 6 SWG G.I wire at 0.50 metre below ground level for conductor earth electrode, including etc. as required.(Sch) 80598 | Mtr | 100 |  |  |
| 15 | Errection, Connection and Testing of Feeder Piller. | Each | 1 |  |  |
| 16 | Febrication, Supply & Fixing of MS feeder Pillar of 16 guage MS sheet, powder coated with following switch gears. | Each | 1 |  |  |
| a | 200 Amps TPN MCCB as Incomer | Each | 1 |  |  |
| B | 100 Amps TPN MCCB as Out going | Each | 2 |  |  |
| c | 63 Amps TPN MCB Isolater | Each | 3 |  |  |
| d | 300 Amps Aluminium Busbar | Each | 1 |  |  |
| e | Indicator Lamp | Each | 1 |  |  |
| f | Amp meter & Volt Meter with selctor switch. | Each | 1 |  |  |
|  |  |  |  |  |  |

vf/k”kklh vfHk;Urk

uxj fuxe] nsgjknwuA