dk;kZy; uxj fuxe] nsgjknwuA

 fufonk lwpuk

 uxj fuxe] nsgjknwu }kjk fuxe ifjlj fLFkr VkÅu gkWy ds fo|qr la;kstu dks mPphd`r djus gsrq 11@0-4 ds0oh0 milaLFkku dk fuekZ.k o ,p0Vh0@,y0Vh0 izksVsDlu fMokbZl vkfn dk;Z djk;s tkus gsrq mRrjk[k.M ds ikoj dkjiksjs”ku@fo|qr lqj{kk funs”kky;@yksd fuekZ.k foHkkx@jkT; vFkok dsUnz ljdkj ds “kkldh;@v)Z”kkldh; foHkkx esa iathd`r Bsdsnkjksa@QeksZ ls fu/kkZfjr izi=ksa ij ßVw&fcMÞ flLVe ij leqfpr :i ls cUn rduhdh o foRrh; fufonk;sa fnukad 16-12-14 dh lka; 3%00 cts rd vkeaf=r dh tkrh gSa] mDr fufonk;s mlh fnu fnukad 16-12-14 dks gh lka;% 4%00 cts [kksyh tka,xhA dsoy rduhdh fufonk esa mRrh.kZ gksus ij gh foRrh; fufonk [kksyh tk;sxhA

 fufonk izi= uxj fuxe] nsgjknwu ds ekxZ izdk”k vuqHkkx rFkk vf/k”kklh vfHk;Urk d{k esa fnukad 22-11-14 dk;kZy; le; ls fnukad 15-12-14 dks iwokZUg 1%00 cts rd fu/kkZfjr “kqYd tek djk dj izkIr fd, tk ldrs gSaA fufonk izi= osc lkbZV nagarnigamdehradun.com ds uxj fuxe fyad ls Hkh izkIr fd;s tk ldrs gSa rFkk e; fufonk “kqYd ds jftLVMZ Mkd@dksfj;j ls fu/kkZfjr le; ls Hksts tk ldrs gSa@fufonk ckDl esa Mkys tk ldrs gSaA Mkd O;oLFkk esa gq, foyEc ij uxj fuxe mRrjnk;h ugh gksxkA rduhdh fcM ds lkFk j{kk/ku layXu djuk vfuok;Z gSA j{kk/ku ys[kkf/kdkjh] uxj fuxe] nsgjknwu ds uke ca/kd gksxkA fdlh Hkh ;k leLr fufonk dks fcuk dkj.k crk;s fujLr djus dk vf/kdkj eq[; uxj vf/kdkjh uxj fuxe nsgjknwu esa fufgr gksxkA

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| dk;Z dk fooj.k | vkax.ku jkf”k | j{kk/ku | fufonk izi= “kqYd  | dk;Z lekfIr vof/k |
| 1. uxj fuxe ifjlj esa 11@0-4 ds0oh0 milLaFkku dk fuekZ.k @,p0Vh0@,y0Vh0 izksVSDlu fMokbZl LFkkfir o vU; fo|qr dk;Z vkfnA
 | 11]29942-00 | 23000-00 | 1000+13-5 % lfoZl VSDl  | ,d ekg |

 eq[; uxj vf/kdkjh

 uxj fuxe] nsgjknwuA

 bZ&esy- nagarnigam2008@yahoo.com

i=kad%& ------------------------@ekxZ iz0@14&15 fnukad%&------------------------

**izfrfyfi%&** izfrfyfi%&

1. ek0 uxj izeq[k]uxj fuxe] nsgjknwuA
2. lEiknd ------------------------------------------------------- dks bl vuqjks/k ds lkFk izsf’kr gS fd mDr fufonk dks layXu izk:i esa izdkf”kr dj fcy ds lkFk lekpkj i= dh nks izfr;ka fu%”kqYd bl dk;kZy; dks izsf’kr djsaA
3. vkbZ0Vh0 vkWfQlj dks bl funsZ”k ds lkFk izsf’kr fd mijksDr fufonk lEcU/kh leLr fooj.k uxj fuxe] nsgjknwu dh osclkbZV nagarnigamdehradun.com ij viyksM djsaA
4. uxj fuxe uksfVl cksMZ gsrqA

 eq[; uxj vf/kdkjh

 uxj fuxe] nsgjknwu

VkÅu gkWy ds ikl VaªklQkeZj vkfn fo|qr dk;Z

¼o’kZ 2014&15½

gsrq

fufonk izi=

fufonk izi= ewY; :0 1000-00++13-50 VSDl

uxj fuxe] nsgjknwu

uxj fuxe] nsgjknwuA

fufonk izi=

:0 1000+13-5 izfr”kr

lfoZl VSDl izfr fufonk

VSfDudy fcM

uxj fuxe ifjlj VkÅu gky ds ikl VªaklQkeZj yxkus vkfn fo|qr dk;Z lEcfU/k

1. ljdkj }kjk ekU;rk izkIr “,” Js.kh ds fo|qr Bsdsnkj dk izek.k i= nsuk gksxkA
2. bUde VSDl] lsy VSDl] iSu uaEcj nsuk gksxk rFkk xr nks o’kksZa dk vk;dj fjVuZ Hkh nsuk gksxkA
3. VªaklQkeZj vkbZ0,l0vkbZ0 ekdZ] dkWij okbZfUMxa rFkk ikoj dkiksZjs”ku }kjk Lohd`r dEiuh dk yxkuk gksxk o nks o’kZ dh xkjUVh nsuh gksxhA
4. lEiw.kZ dk;Z dh ,d o’kZ rd fu%”kqYd eSUVsusUl djuh gksxhA
5. dsfcy gSoYl] ikSyhdSc] ikbZeu dk yxkuk gksxkA
6. ,e0lh0ch0@,e0lh0lh0ch0 vkfn gSoYl] ,y0 ,.M Vh0 dh yxkuh gksxhA
7. foxr nks o’kksZa dk VuZ vksoj :0 chl yk[k ds fo|qr lEcfU/kr dk;ksZa dk izek.k i= nsuk gksxkA
8. rduhdh fcM o foRrh; fcM vyx&vyx fyQkQs esa nsuh gksxh rFkk nksuks fcMksa dks ,d cMs fyQkQs esa lhy cUn djds nsuk gksxkA
9. rduhdh fcM esa lQy gksus okys fufonknkrk dh gh foRrh; fcM [kksyh tk;sxhA
10. tekur /kujkf”k :0 23000-00 dh lh0Mh0vkj0@,Q0Mh0vkj0 ,d o’kZ dh oS|rk ds lkFk ys[kkf/kdkjh uxj fuxe nsgjknwu ds uke VSfDudy fcM ds lkFk nsuh vfuok;Z gS] vU;Fkk fufonk ij fopkj ugh fd;k tk;sxkA
11. fujh{kd fo|qr lqj{kk mRrjk[k.M }kjk tkjh Hkkj voeqfDr gsrq djk;s x;s ,p0Vh0 dk;ksZa dh fujh{k.k vk[;k izLrqr djuh gksxhA

vf/k”kklh vfHk;Urk

uxj fuxe] nsgjknwuA

Nagar Nigam, Dehra dun

Fininancial Bid

 Fininancial Bid of Construction of Various Plinths for Errection of Transformer & Panel Board.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr No | Description | Dimension | Qty | Unit | Rate | Amount. |
| 1 | Excavation work | 1x2.75x2.25x0.30 | 1.86 | Cum |  |  |
| 2.a | PCC work | 2x2.75x0.45x0.075 | 0.19 | Cum |  |  |
| 2.b | PCC work | 2x2.25x0.45x0.075 | 0.15 | Cum |  |  |
| 3.a | Brick Work | 2x2.50x0.90x0.23 | 1.035 | Cum |  |  |
| 3.b | Brick Work | 2x1.54x0.90x0.23 | 0.638 | Cum |  |  |
| 4.a | Plaster | 2x2.50x0.90 | 4.5 | 7 |  |  |
| 4.b | Plaster | 2x2.00x0.90 | 3.6 | Sqm |  |  |
| 5 | Return Earth Filling | 1x1.56x2.04x0.90 | 2.86 | Cum |  |  |
| 6 | RCC | 1x2.5x2x0.15 | 0.75 | Cum |  |  |
| 7.a | TMT Bar 10 sqmm | 26x2x0.60 | 31.35 | Kg |  |  |
| 7.b | TMT Bar 10 sqmm | 21x2.50x0.60 | 31.35 | Kg |  |  |
|  |  |  |  |  |  |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sr No | Description | Dimension | Qty | Unit | Rate | Amount. |
| 1 | Excavation work | 0.90x0.75x0.30 | 0.2 | Cum |  |  |
| 2 | PCC work | 2x0.90x0.45x0.075 | 0.061 | Cum |  |  |
| 3.a | Brick Work | 2x0.750x0.90x0.23 | 0.31 | Cum |  |  |
| 3.b | Brick Work | 2x0.14x0.90x0.23 | 0.06 | Cum |  |  |
| 4 | PCC work | 0.60x0.90x0.15 | 0.0815 | Cum |  |  |
| 4a | Plaster | 2x0.75x0.90 | 1.35 | Sqm |  |  |
| 4b | Plaster | 2x0.60x0.90 | 1.08 | Sqm |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |

vf/k”kklh vfHk;Urk

uxj fuxe] nsgjknwuA

**--2--**

Nagar Nigam, Dehra dun

 Fininancial Bid for Leying of XLPE Aromored Cable of Various Size & SITC of Electrical Panel Board.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Sr No | Description | Qty | Unit | Rate | Amount. |
| 1 | Supply & Leying of 11 KV, 3X120 sqmm HT aluminum cable armored, XLPE seathed in trench with brick, sand for coushning. | 10 | Mtr |  |  |
| 2 | Supply & Leying of 1100 V,3.5X120 sqmm aluminum cable Armored, XLPE seathed in trench with brick, sand for coushning. 5101(R)(A) | 100 | Mtr |  |  |
| 3 | Supply & Leying of 1100 V,3.5X70 sqmm aluminum cable Armored, XLPE seathed in trench with brick, sand for coushning. (P) | 210 | Mtr |  |  |
| 4 | Supply & Leying of 1100 V,3.5X50 sqmm aluminum cable Armored, XLPE seathed in trench with brick, sand for coushning. (O) | 110 | Mtr |  |  |
| 5 | Supply & Leying of 1100 V,3.5X50 sqmm aluminum cable Armored, XLPE seathed in trench with brick, sand for coushning. (C) | 100 | Mtr |  |  |
| 6 | HT outdoor joint from 70 to 120 sqmm for HT cable. | 2 | Nos |  |  |
|  |  |  |  |  |  |
|  | **Fabrication of outdoor electrical** |  |  |  |  |
| 1 | Distribution panel borard with MS sheet & powder coated. | 1 | Nos |  |  |
| 1.a | Incoming thermal magnetic & micro proceser release MCCB 4 pol 400 Amp (35k) | 1 | Nos |  |  |
| 1.b | Outgoing thermo magnetic proceser MCCB 4 pole 200 Amp  | 1 | Nos |  |  |
| 1.c | Outgoing thermo magnetic proceser MCCB 4 pole 100 Amp | 5 | Nos |  |  |
| 1.d | 4 pole 63 Amp MCCB | 2 | Nos |  |  |
| 1.e | 4 pole single pole MCCB 40 Amp | 4 | Nos |  |  |
| 1.f. | Amp meter, Volt meter with selector switch Supply of factory febriacted, powder coated, | 2 | Set |  |  |
| 2. | MS terminal Box with 200+100 Amps TPN Busbar. Cable End termination of 120 sqmm. | 3 | Nos |  |  |
| 3. | Aluminum armoured XLPE cable with Aluminum Lugs & Cable glands. Cable Eng termination of 70 sqmm. | 2 | Set |  |  |
| 4. | Aluminum armoured XLPE cable with Aluminum Lugs & Cable glands.  | 6 | Set |  |  |
| 5. | EARTHING 600x600x6m G.L full earthing | 2 | Nos |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

vf/k”kklh vfHk;Urk

uxj fuxe] nsgjknwuA

**--3--**

Nagar Nigam, Dehra dun

Fininancial Bid for SITC of 11KV 440 V Transformer.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Sr No | Description | Qty | Unit | Rate | Amount. |
| 1 | Supply, Installation, Testing & Commissioning of 11 KV 250 KVA 11000/440 VoltAC, 3 phase. 3 phase & Nutral LT supply. | 1 | Job |  |  |
| 2 | Supply & Errection of swaged MS Tubular pole 9.5 mtr long, with proper concreting & plinth. | 2 | Nos |  |  |
| 3 | Supply, Installation, Testing & Commissioning of 3 phase, 11 KV Gang Operated Switch, with 3 nos 11 kv fuse set. | 1 | Nos |  |  |
| 4 | S@B of 600X600X6mm G.I Plate vertically forearthing with its top at least 3.5 mtr below ground level. Complete in all respect. | 2 | Nos |  |  |
|  |  |  |  |  |  |

vf/k”kklh vfHk;Urk

uxj fuxe] nsgjknwuA